 **OPERATION SHEET**

**SNORKEL**

**BASIC SET UP GUIDE**

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Snorkle Basic Set up Guide. | | | | |  |  |  |  |  |  |  |  |  |
| Step 1 Remove trailer boom from vehicle. | | | | |  |  |  |  |  |  |  |  |  |
| Step 2 Remove front locking travel pin | | | |  |  |  |  |  |  |  |  |  |  |
| Step 3 Undo rear travel latch | | |  |  |  |  |  |  |  |  |  |  |  |
| Step 4 Check Fuel tank is full | | |  |  |  |  |  |  |  |  |  |  |  |
| Step 5 Put Key in ignition and select base contol position | | | | | |  |  |  |  |  |  |  |  |
| Step 6 Hold choke switch and start engine | | | | |  |  |  |  |  |  |  |  |  |
| Step 7 Lower front stabilizers and lift front of machine so jockey wheel is off the ground. | | | | | | | | |  |  |  |  |  |
| Step 8 Lower rear stabilizers so wheels are of the ground | | | | | |  |  |  |  |  |  |  |  |
| Step 9 Press self leveling button located near stabilizer manual operation switches. | | | | | | | | |  |  |  |  |  |
| Step 10 Make sure all green lights are visible on stabilizer control panel indicating machine is level. | | | | | | | | | |  |  |  |  |
| Step 11 Switch key to upper control position. | | | | |  |  |  |  |  |  |  |  |  |
| Step 12 Fit safety harness. | | |  |  |  |  |  |  |  |  |  |  |  |
| Step 13 Enter basket and attach harnes to basket base lug. | | | | | |  |  |  |  |  |  |  |  |
| Step 14 Check surroundings for safe operation before haising basket. | | | | | | |  |  |  |  |  |  |  |
| Step 15 Place foot on dead man pedal. | | | |  |  |  |  |  |  |  |  |  |  |
| Step 16 Lift lower boom in conjunction with upper boom past slew lock out height. | | | | | | | |  |  |  |  |  |  |
| Step 17 Upon lowering back to ground ensure machine slew is back to rear central position and a green centering light will appear on the upper control panel. | | | | | | | | | | | | | |
| Step 19 Ensure both travel locking pins are in place before transporting. | | | | | | |  |  |  |  |  |  |  |
| Step 20. Ensure tow hitch is locked in place, light plud and safety chaind are in place and basket is free of tools , harness etc. | | | | | | | | | | | |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| NB. This is a guide only. It is recommended that all users are familiar with the operators handbook located in the pouch fixed to the basket. | | | | | | | | | | | | | |

**Please refer to the User Guide and Operators Manual**

**for detailed Operating Instructions**

*The safety information contained in this assessment is general information only and should not be relied upon as a substitute for professional advice or tuition, which the hirer should seek before operating.*