All lights and reflectors are present and serviceable (if fitted, machines without lights must only be used during daylight hours)

Engine oil level OK COMMENTS:

Hydraulic oil level OK COMMENTS:

Coolant level OK COMMENTS:

AdBlue level OK COMMENTS:

Fuel level OK COMMENTS:

Machine free from major leaks to engine, cooling system, hydraulics, drive line etc. COMMENTS:

Fire extinguisher is present & within inspection period COMMENTS:

**PRE START - EXTERNAL INSPECTION**

**PRE START - FLUIDS**

# COMMENTS:

Amber safety beacon is fully functional COMMENTS:

All hydraulic hoses are connected properly and free from leaks and damage (never use your hand to check for leaks, use wood or card board)

# COMMENTS:

Hydraulic cylinder(s) free from leaks and damage COMMENTS:

All batteries are constrained & fitted with a sturdily attached cover COMMENTS:

All engine & exhaust guards are present, sturdily attached and free from damage COMMENTS:

All tracks and track components are in safe working condition COMMENTS:

Quick hitch (if fitted) fitted with locking pins, retainers & retention device in a safe working condition (consider excessive wear, cracks etc.)

# COMMENTS:

All grease points present, functional and greased as per manufacturer's recommendations COMMENTS:

All structural components are in safe working condition COMMENTS:

All operator access is non slip, sturdily attached and free from damage with three points of contact available COMMENTS:

Operator floor is non slip, free from damage & rubbish COMMENTS:

All items in cabin/work area that could cause harm to the operator are securely restrained COMMENTS:

Seat(s) sturdily attached and free from damage COMMENTS:

Seat belt(s) present, sturdily attached and free from damage COMMENTS:

Two mirrors fitted & fully functional (one on each side of machine) COMMENTS:

All windows and screens are present, clean and free from damage COMMENTS:

**PRE START - OPERATOR WORK AREA**

Two exits available (vandal proof guarding removed) COMMENTS:

Windscreen wipers are present, free from damage & fully functional COMMENTS:

Air conditioning/heating fully functional COMMENTS:

Operator warning device (horn) is fully functional COMMENTS:

All controls are fully functional, free from damage and clearly and legibly labelled as to purpose and method of operation

# COMMENTS:

Movement awareness alarm present & fully functional COMMENTS:

Overhead power line minimum approach distance table present & legible COMMENTS:

"Dial Before You Dig" warning label present and legible COMMENTS:

Machine functions as per manufacturer's operating instructions COMMENTS:

Load chart present & legible (for machines with a lifting point) COMMENTS:

All lifting components (wire ropes, chains, hooks, slings etc.) are free from damage COMMENTS:

Manufacturer's operational and safety information is available COMMENTS:

**PRE START - OTHER**

**PRE START - INFORMATION**

**PRE START - LIFTING**

**PRE START - MACHINE FUNCTION**

Is this item of plant free from any other safety fault which requires attention, if No then document issue in comments section.

# COMMENTS:

**Inspected By: Inspected On: Signature:**